module Base
{
	recipe Repair Ford CVPI Tire
    	{
		fordCVPITire1,
		damnCraft.TireRepairTools,
		damnCraft.TireRepairRubberSolution,
		damnCraft.TireRepairStrips,

		NoBrokenItems:false,
		Result:damnCraft.TireRepairTools,
		Time:250.0,
		OnCreate:DAMN.OnCreate.RepairTire,
		NeedToBeLearn:false,
		CanBeDoneFromFloor:true,
    }

    recipe Repair 91 Ford LTD Tire
    	{
		91fordLTDTire1,
		damnCraft.TireRepairTools,
		damnCraft.TireRepairRubberSolution,
		damnCraft.TireRepairStrips,

		NoBrokenItems:false,
		Result:damnCraft.TireRepairTools,
		Time:250.0,
		OnCreate:DAMN.OnCreate.RepairTire,
		NeedToBeLearn:false,
		CanBeDoneFromFloor:true,
    }

	fixing Fix 91 Ford LTD Seat
	{
	   Require : 91fordLTDSeatFront1;91fordLTDSeatRear1,
	   ConditionModifier : 0.5,

       Fixer : DuctTape=2;Mechanics=1,
	}
	
	fixing Fix 91 Ford LTD Trunk Welding
	{
	   Require : 91fordLTDTrunk1;91fordLTDWagonTrunk1;91fordLTDRoofrack1,
	   GlobalItem : BlowTorch=5,
	   ConditionModifier : 1.2,

       Fixer : SheetMetal; MetalWelding=3;Mechanics=2,
       Fixer : SmallSheetMetal=2; MetalWelding=3;Mechanics=2,
	}

	fixing Fix 91 Ford LTD Hood Welding
	{
	   Require : 91fordLTDEngineDoor1,
	   GlobalItem : BlowTorch=5,
	   ConditionModifier : 1.2,

       Fixer : SheetMetal; MetalWelding=1;Mechanics=2,
       Fixer : SmallSheetMetal=2; MetalWelding=1;Mechanics=2,
	}

   fixing Fix 91 Ford LTD Hood
	{
	   Require : 91fordLTDEngineDoor1,
	   GlobalItem : Screws=8,
	   ConditionModifier : 0.5,

       Fixer : SheetMetal; Mechanics=2,
	}

	fixing Fix 91 Ford LTD Trunk Lid Welding
    {
       Require : 91fordLTDTrunkDoor1;91fordLTDWagonTrunkDoor1,
       GlobalItem : BlowTorch=5,
       ConditionModifier : 1.2,

       Fixer : SheetMetal; MetalWelding=1;Mechanics=2,
       Fixer : SmallSheetMetal=2; MetalWelding=1;Mechanics=2,
    }

   fixing Fix 91 Ford LTD Trunk Lid
	{
      Require : 91fordLTDTrunkDoor1;91fordLTDWagonTrunkDoor1,
	   GlobalItem : Screws=8,
	   ConditionModifier : 0.5,

       Fixer : SheetMetal; Mechanics=2,
	}

	fixing Fix 91 Ford LTD Door Welding
	{
	   Require : 91fordLTDFrontDoor1;91fordLTDRearDoor1,
	   GlobalItem : BlowTorch=5,
	   ConditionModifier : 1.2,

       Fixer : SheetMetal; MetalWelding=3;Mechanics=3,
       Fixer : SmallSheetMetal=2; MetalWelding=3;Mechanics=3,
	}

	fixing Fix Ford CVPI Armor Welding
    {
       Require : fordCVPIWindshieldArmor;fordCVPIFrontWindowArmor;fordCVPIRearWindowArmor;fordCVPIWindshieldRearArmor,
       GlobalItem : BlowTorch=8,
       ConditionModifier : 1.0,

       Fixer : SheetMetal; MetalWelding=4;Mechanics=4,
       Fixer : SmallSheetMetal=2; MetalWelding=4;Mechanics=4,
    }

	fixing Fix 91 Ford LTD Armor Welding
    {
       Require : 91fordLTDBumperFront1;91fordLTDWagonBackWindowArmor;91fordLTDWagonWindshieldRearArmor;91fordLTDCabBarrier1,
       GlobalItem : BlowTorch=7,
       ConditionModifier : 1.0,

       Fixer : SheetMetal; MetalWelding=4;Mechanics=4,
       Fixer : SmallSheetMetal=2; MetalWelding=4;Mechanics=4,
    }

    fixing Fix 91 Ford LTD Plastic Welding
    {
       Require : 91fordLTDBumperFront0;91fordLTDBumperRear0;91fordLTDWagonBumperRear1,
       GlobalItem : PlasticWeldingGun=250,
       ConditionModifier : 0.85,

       Fixer : PlasticWeldingStaples100Pack; Mechanics=4,
    }

}
